,Weight##MASS##KILOGRAMS,Height##LENGTH##MILLIMETERS,Material housing##OTHER##,Dimming type option##OTHER##,Luminaire mounting type##OTHER##,LED source##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Height 2##LENGTH##MILLIMETERS,Etim class##OTHER##,IP code##OTHER##,Article number##OTHER##,Impact strength##OTHER##,Utility frequency##OTHER##,Power input##ELECTRICAL_WATTAGE##WATTS,Nominal current##ELECTRICAL_CURRENT##AMPERES,Width##LENGTH##MILLIMETERS,Energy class##OTHER##,Shape##OTHER##,Protection class##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Manufacturer##OTHER##,Product URL##OTHER##,Created by##OTHER##
LADOR 1 - LD-50002 - 1 LED - 4 W - 34° - RGBW40 - DMX/RDM,0.7,62,Aluminium,DMX/RDM,surface ceiling mounted,1,170,43,Downlight/spot/floodlight,IP66,LD-50002-M-40-DMXRDM,IK08,24,4,24,62,A,square,III,220,LIGMAN,,https://bimproject.cloud
LADOR 1 - LD-50002 - 1 LED - 4 W - 34° - RGBW30 - DMX/RDM,0.7,62,Aluminium,DMX/RDM,surface ceiling mounted,1,166,43,Downlight/spot/floodlight,IP66,LD-50002-M-30-DMXRDM,IK08,24,4,24,62,A,square,III,220,LIGMAN,,https://bimproject.cloud