,Article number##OTHER##,Material housing##OTHER##,Dimming type option##OTHER##,Luminaire mounting type##OTHER##,Weight##MASS##KILOGRAMS,LED source##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Etim class##OTHER##,Height##LENGTH##MILLIMETERS,IP code##OTHER##,Impact strength##OTHER##,Utility frequency##OTHER##,Nominal current##ELECTRICAL_CURRENT##AMPERES,Energy class##OTHER##,Length##LENGTH##MILLIMETERS,Shape##OTHER##,Power input##ELECTRICAL_WATTAGE##WATTS,Protection class##OTHER##,Width##LENGTH##MILLIMETERS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Manufacturer##OTHER##,Product URL##OTHER##,Created by##OTHER##
LADOR 2 - LD-50012 - 4 LED - 10 W - 43°x11° - RGBW30 - DMX/RDM,LD-50012-E-30-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,466,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 43°x11° - RGBW40 - DMX/RDM,LD-50012-E-40-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,475,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 17° - RGBW30 - DMX/RDM,LD-50012-M-30-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,430,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 17° - RGBW40 - DMX/RDM,LD-50012-M-40-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,440,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 8° - RGBW30 - DMX/RDM,LD-50012-N-30-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,508,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 8° - RGBW40 - DMX/RDM,LD-50012-N-40-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,520,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 65° - RGBW30 - DMX/RDM,LD-50012-VW-30-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,406,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 65° - RGBW40 - DMX/RDM,LD-50012-VW-40-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,416,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 26° - RGBW30 - DMX/RDM,LD-50012-W-30-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,446,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud
LADOR 2 - LD-50012 - 4 LED - 10 W - 26° - RGBW40 - DMX/RDM,LD-50012-W-40-DMXRDM,Aluminium,DMX/RDM,surface ceiling mounted,1,1,458,Downlight/spot/floodlight,82,IP66,IK08,24,24,A,82,rectangle,10,III,43,220,LIGMAN,,https://bimproject.cloud