,Power input##ELECTRICAL_WATTAGE##WATTS,Length##LENGTH##MILLIMETERS,Material housing##OTHER##,Height 2##LENGTH##MILLIMETERS,Nominal current##ELECTRICAL_CURRENT##AMPERES,Dimming type option##OTHER##,Luminaire mounting type##OTHER##,Article number##OTHER##,LED source##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Etim class##OTHER##,IP code##OTHER##,Impact strength##OTHER##,Weight##MASS##KILOGRAMS,Height##LENGTH##MILLIMETERS,Energy class##OTHER##,Shape##OTHER##,Width##LENGTH##MILLIMETERS,Protection class##OTHER##,Utility frequency##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Manufacturer##OTHER##,Product URL##OTHER##,Created by##OTHER##
LADOR 4 - LD-50032 - 16 LED - 28 W - 43°x11° - RGBW30 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-E-30-DMXRDM,1,1493,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 43°x11° - RGBW40 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-E-40-DMXRDM,1,1540,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 17° - RGBW30 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-M-30-DMXRDM,1,1373,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 17° - RGBW40 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-M-40-DMXRDM,1,1417,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 8° - RGBW30 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-N-30-DMXRDM,1,1551,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 8° - RGBW40 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-N-40-DMXRDM,1,1600,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 65° - RGBW30 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-VW-30-DMXRDM,1,1322,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 65° - RGBW40 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-VW-40-DMXRDM,1,1364,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 26° - RGBW30 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-W-30-DMXRDM,1,1387,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud
LADOR 4 - LD-50032 - 16 LED - 28 W - 26° - RGBW40 - DMX/RDM,28,145,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50032-W-40-DMXRDM,1,1431,Downlight/spot/floodlight,IP66,IK08,3,145,A,rectangle,120,I,50,220,LIGMAN,,https://bimproject.cloud