,Material housing##OTHER##,Height 2##LENGTH##MILLIMETERS,Nominal current##ELECTRICAL_CURRENT##AMPERES,Dimming type option##OTHER##,Luminaire mounting type##OTHER##,Article number##OTHER##,LED source##OTHER##,Length##LENGTH##MILLIMETERS,Weight##MASS##KILOGRAMS,Etim class##OTHER##,IP code##OTHER##,Impact strength##OTHER##,Width##LENGTH##MILLIMETERS,Energy class##OTHER##,Power input##ELECTRICAL_WATTAGE##WATTS,Shape##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Protection class##OTHER##,Height##LENGTH##MILLIMETERS,Utility frequency##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Manufacturer##OTHER##,Product URL##OTHER##,Created by##OTHER##
LADOR 3 - LD-50022 - 8 LED - 22 W - 43°x11° - RGBW30 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-E-30-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,988,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 43°x11° - RGBW40 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-E-40-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,1019,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 17° - RGBW30 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-M-30-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,927,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 17° - RGBW40 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-M-40-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,957,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 8° - RGBW30 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-N-30-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,1098,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 8° - RGBW40 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-N-40-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,1133,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 65° - RGBW30 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-VW-30-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,853,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 65° - RGBW40 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-VW-40-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,880,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 26° - RGBW30 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-W-30-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,919,I,120,50,220,LIGMAN,,https://bimproject.cloud
LADOR 3 - LD-50022 - 8 LED - 22 W - 26° - RGBW40 - DMX/RDM,Aluminium,50,230,DMX/RDM,surface ceiling mounted,LD-50022-W-40-DMXRDM,1,120,2,Downlight/spot/floodlight,IP66,IK08,110,A,22,rectangle,949,I,120,50,220,LIGMAN,,https://bimproject.cloud